UDC 621.433:621.436.068

Parsadanov I.V. Implementation of water-fuel emulsion in autotrector diesel. Eciological efficiency (Part 1) / I.V.

Parsadanov, A.A. Teplizkoj, V.V. Solodovnikov, S.U. Belik // Internal combustion engines. – 2011. – № 2. – P.

118-121.

The estimation of the changing in autotractor diesel’s

ecological indexes during the work on water-fuel emulsion is

given. Findings of investigation has shown that implementation

of water-fuel emulsion on basis of diesel fuel with emulsifier

which provids long-term storage allows to reduce emission

in diesel engine under the same power without changing

in diesel’s construction and adjustment. Table. 1. Il. 5. Bibliogr.

5 names.